
==================================================
PL-2303 CheckChipVersion Tool Program v1.0.0.6
For Windows OS Only
==================================================

System Requirement:
  . USB 1.1/2.0/3.0 Host Controller
  . Device using PL2303HX/X/EA/RA/SA/TA/TB version chips
  . PL-2303 Windows Driver Installer v1.8.0 or above
  . Supports the following Windows OS Family:
	- Windows XP SP2 and above (32 & 64 bit)
	- Windows Vista (32 & 64 bit)
	- Windows 7 (32 & 64 bit)
	- Windows 8/8.1/10 (32 & 64 bit) 
	NOTE: 
	  - Windows 8 is NOT supported in HXA/XA chip versions (will show yellow mark Error Code 10).
	  - Windows 8 is supported only in following chip versions:
	      - PL2303HXD (HX Rev D)
	      - PL2303EA (ESD protection)
	      - PL2303RA (Built-in transceiver)
	      - PL2303SA (SOP8 package)
	      - PL2303TA (PL2303HXA/XA replacement)
	      - PL2303TB (12 GPIO)
 
Supported device ID and product strings:
  . VID_067B&PID_2303 for "Prolific USB-to-Serial Comm Port"
  . VID_067B&PID_2304 for "Prolific USB-to-Serial Comm Port" (PL2303TB chip)
  . Other VID/PID based on PL2303 chip. 



